**Nevada Standards Laboratory**

**Preparation of Large Volume Provers for Calibration**

In order to have your prover(s) calibrated, we require that they be cleaned before being brought to our facility. We ask that you clean all surfaces (inside and out), drain lines, pumps, and hoses that may be used during the calibration process so that no petroleum or other product residue remains that would otherwise spill onto the asphalt surface of the testing bay or pour into the sewer system. Also do not use soap since it will add air bubbles to the prover negatively impacting the calibration.

We require your certification that this has been done before we will test your prover(s). Please complete the bottom portion of this form for each prover that you are submitting for calibration.

**Prover Cleanliness Certification**

|  |  |
| --- | --- |
| **Prover Manufacturer:** | **Prover ID (Serial No):** |
| **Prover Volume** | **Graduation Size** |
| **Material** *(circle which one)* | Stainless Steel or Mild Steel or Aluminum |
| **Owner’s Name:** | |
| **Address:** | |
| **Telephone Number** | **Email Address** |
| **I certify that this prover has been cleaned so that there is no petroleum or other product residue remaining on or in the prover, drain lines, pumps, or hoses.** | |
| **Signature:**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** | **Date:**  **\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_** |
| **Printed Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  ***Present this signed form to the Metrologist on the day of calibration.*** | |